Previous: tinc, Up: Introduction [Contents][Index]

### 1.3 Supported platforms

Tinc has been verified to work under Linux, FreeBSD, OpenBSD, NetBSD, MacOS/X (Darwin), Solaris, and Windows (both natively and in a Cygwin environment), with various hardware architectures. These are some of the platforms that are supported by the universal tun/tap device driver or other virtual network device drivers. Without such a driver, tinc will most likely compile and run, but it will not be able to send or receive data packets.

For an up to date list of supported platforms, please check the list on our website: http://www.tinc-vpn.org/platforms/.